**Hazard Communication Standard Labels**

OSHA updated the requirements for labeling of hazardous chemicals under its Hazard Communication Standard (HCS). Manufacturer’s labels are required to have pictograms, a signal word, hazard and precautionary statements, the product identifier, and supplier identification. A sample revised Hazard Communication Standard label, identifying the required label elements, is shown below. Supplemental information can also be provided on the label as needed.

Contact PIM for help or more information regarding Hazard Communication or any other Safety or Environmental question you might have.

* Paul Gutkowski at paulg@pimw.org, 612-400-6205 or
* Cathy Malinowski at cathym@pimw.org, 612-868-6771